#
CONDENSER REMOVAL/INSTALLATION

id071100801200

1. Disconnect the negative battery cable.

2. Discharge the refrigerant from the system. (See REFRIGERANT RECOVERY.) (See REFRIGERANT CHARGING.)

3. Remove the shroud panel. (See SHROUD PANEL REMOVAL/INSTALLATION.)

  Caution

  • If moisture or foreign material enters the refrigeration cycle, cooling ability will be lowered and abnormal noise will occur. Always immediately plug all open fittings after removing any refrigeration cycle parts to keep moisture or foreign material out of the cycle.

4. Remove in the order indicated in the table. Do not allow compressor oil to spill.

1 | Cooler pipe No.1 (See Refrigerant Lines Removal Note.) (See Refrigerant Lines Installation Note.)
2 | Cooler pipe No.2 (See Refrigerant Lines Removal Note.) (See Refrigerant Lines Installation Note.)
3 | Condenser (See Condenser Installation Note.)

5. Install in the reverse order of removal.

6. Perform the refrigerant system performance test. (See REFRIGERANT SYSTEM PERFORMANCE TEST.)

## Condenser Installation Note

1. When installing a new condenser, add a supplemental amount of ATMOS GU10 compressor oil inlet the refrigerant cycle.

Supplemental amount (approx. quantity)

  35 ml {35 cc, 1.2 fl oz}