#
PID/DATA MONITOR TABLE [HEADLIGHT AUTO LEVELING SYSTEM]

id0902i7862100

## LHID

PID Name (Definition) | Unit/Condition | Condition/Specification | Auto Leveling Control Module (Main) terminal
--- | --- | --- | ---
CCNT (Number of continuous codes) | - | • DTC is detected: 1-255 • DTC is not detected: 0 | -
ONDEMDTC (Number of on-demand codes) | - | • DTC is detected: 1-255 • DTC is not detected: 0 | -
LHIDIGNV (Auto leveling control module (main) input voltage) | VOLTAGE | Ignition switch at ON: B+ | L
F_CAL (Signal input from front auto leveling sensor at time of headlight zeroset (stored in memory)) | VOLTAGE | Ignition switch at ON: 0.5-4.5 V | -
F_LEVEL (Current input signal sent from front auto leveling sensor) | VOLTAGE | Ignition switch at ON: 0.5-4.5 V | G,H,K
R_CAL (Signal input from rear auto leveling sensor at time of headlight zeroset (stored in memory)) | VOLTAGE | Ignition switch at ON: 0.5-4.5 V | -
R_LEVEL (Current input signal sent from rear auto leveling sensor) | VOLTAGE | Ignition switch at ON: 0.5-4.5 V | F,G,K
L_REFLECTOR (Headlight leveling actuator angle control output signal sent to auto leveling control module (sub)) | ANGLE | Ignition switch at ON: -5-4 | I
STP_MTR_L (Headlight leveling actuator (LH) current position) | STEP | Ignition switch at ON: 12-520 | Q,R,S,T
LHID_VSS (Vehicle speed input signal from ABS/TCS HU/CM) | KPH | • Vehicle is stopped: 0 KPH {0 MPH} • Vehicle is driving: Indicates vehicle speed | P
PART#SUF* (Part number identification should be displayed) | - | - | -
SERIAL#1* (Auto leveling control module serial number part 1 should be displayed) | - | - | -
SERIAL#2* (Auto leveling control module serial number part 2 should be displayed) | - | - | -
SOFTVER* (Software version number should be displayed) | - | - | -
L_VOLT_L (Discharge headlight control (LH) input voltage) | VOLTAGE | Headlight switch at ON: B+ | D
GDL_P_L (Output power to discharge headlight bulb (LH)) | WATT | Headlight switch at ON: 35-65 W | -
GDL_V_L (Output voltage to discharge headlight bulb (LH)) | VOLTAGE | Headlight switch at ON: 68-112 V | -

  * :
Unnecessary for diagnosis

## RHID

PID Name (Definition) | Unit/Condition | Condition/Specification | Auto Leveling Control Module (Sub) terminal
--- | --- | --- | ---
CCNT (Number of continuous codes) | - | • DTC is detected: 1-255 • DTC is not detected: 0 | -
ONDEMDTC (Number of on-demand codes) | - | • DTC is detected: 1-255 • DTC is not detected: 0 | -
RHIDIGNV (Auto leveling control module (sub) input voltage) | VOLTAGE | Ignition switch at ON: B+ | L
R_REFLECTOR (Headlight leveling actuator angle control input signal sent from auto leveling control module (main)) | ANGLE | Ignition switch at ON: -5-4° | P
STP_MTR_R (Headlight leveling actuator (RH) current position) | STEP | Headlight switch at ON: 12-520 | Q,R,S,T
PART#SUF* (Part number identification should be displayed) | - | - | -
SERIAL#1* (Auto leveling control module serial number part 1 should be displayed) | - | - | -
SERIAL#2* (Auto leveling control module serial number part 2 should be displayed) | - | - | -
SOFTVER* (Software version number should be displayed) | - | - | -
L_VOLT_R (Discharge headlight control module (RH) input voltage) | VOLTAGE | Headlight switch at ON: B+ | D
GDL_P_R (Output power to discharge headlight bulb (RH)) | WATT | Headlight switch at ON: 35-65 W | -
GDL_V_R (Output voltage to discharge headlight bulb (RH)) | VOLTAGE | Headlight switch at ON: 68-112 V | -

  * :
Unnecessary for diagnosis