PRIMARY SHAFT COMPONENTS DISASSEMBLY

id051500803000

1. Disassemble in the order indicated in the table.

bmgezm00000001

1 | Bearing (4th gear end) (See Bearing (4th Gear End) Disassembly Note.)
2 | 4th gear
3 | Inner cone
4 | Double cone
5 | 4th synchronizer ring
6 | Retaining ring
7 | Sleeve
8 | Ball
9 | 3rd/4th clutch hub component (See 3rd/4th Clutch Hub Component, 3rd Synchronizer Ring and 3rd Gear Disassembly Note.)
10 | 3rd synchronizer ring (See 3rd/4th Clutch Hub Component, 3rd Synchronizer Ring and 3rd Gear Disassembly Note.)
11 | Double cone
12 | Inner cone
13 | 3rd gear (See 3rd/4th Clutch Hub Component, 3rd Synchronizer Ring and 3rd Gear Disassembly Note.)
14 | Bearing (primary shaft end) (See Bearing (Primary Shaft End) Disassembly Note.)
15 | Primary shaft gear
16 | Synchronizer key spring
17 | 3rd/4th clutch hub sleeve
18 | Synchronizer key
19 | 3rd/4th clutch hub

Bearing (4th Gear End) Disassembly Note

1. Remove the bearing using the SST.

bmgezm00000002

3rd/4th Clutch Hub Component, 3rd Synchronizer Ring and 3rd Gear Disassembly Note

1. Remove the retaining ring.

2. Remove the 3rd/4th clutch hub component, 3rd synchronizer ring, double cone, inner cone, and 3rd gear using the SST.

bmgezm00000003

Bearing (Primary Shaft End) Disassembly Note

1. Remove the bearing using the SST.

bmgezm00000004

  Caution
  • Use protective plates in the vise to prevent damage to the primary shaft gear.