#
POWER WINDOW MOTOR REMOVAL/INSTALLATION

id091200416900

1. Disconnect the negative battery cable.

2. Remove the front door trim or rear door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.) (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

3. Disconnect the power window motor connector.

4. Remove the bolts.

5. Remove the power window motor from the power window regulator drum.

6. Install in the reverse order of removal.

  Note

  • When installing the power window motor to the power window regulator drum, the drum housing hook may come off the door unit. If this happens, remove the door speaker, insert your hand in the speaker installation hole, connect the drum housing hooks, and while supporting the drum housing, install the power window motor to the drum.