#
REAR BELTLINE MOLDING REMOVAL

id091600800500

  Note

  • When removing the rear beltline molding, the clip may be damaged. If the clip is damaged, replace it with a new one.

1. Pull the A section upward and remove the clip.

2. Rotate the B section of the front beltline molding in direction (2), along the direction (1) shown in the figure and remove it from the body.

3. Pull the C section upward and remove the clip. Then remove the front beltline molding.