#
TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR REMOVAL/INSTALLATION [JA5AX-EL]

id051705801100

1. Remove the automatic transaxle. (See AUTOMATIC TRANSAXLE AND TRANSFER REMOVAL/INSTALLATION [JA5AX-EL].)

2. Disassemble the automatic transaxle, and then remove the TFT sensor. (See Automatic Transaxle Workshop Manual JA5A-EL)

3. Install a TFT sensor, and then assemble the automatic transaxle. (See Automatic Transaxle Workshop Manual JA5A-EL)

4. Install the automatic transaxle. (See AUTOMATIC TRANSAXLE AND TRANSFER REMOVAL/INSTALLATION [JA5AX-EL].)

5. Carry out the line pressure test. (See Line Pressure Test.)

6. Inspect the operation of the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5AX-EL].)

7. Inspect the operation of the selector lever. (See SELECTOR LEVER INSPECTION.)

8. Carry out the mechanical system test. (See MECHANICAL SYSTEM TEST [JA5AX-EL].)

9. Carry out the road test. (See ROAD TEST [JA5AX-EL].)