#
WHEEL AND TIRE SPECIFICATION

id021200800100

  European (L.H.D. U.K.) specs.

  Item | Specification
  --- | ---
  Standard tire and wheel
  Wheel | Size | 15 × 6J | 16 × 7J | 17 × 7J | 18 × 7J
  Offset | (mm {in}) | 50 {1.97} | 55 {2.17}
  Pitch circle diameter | (mm {in}) | 114.3 {4.50}
  Material | Steel | Aluminum alloy
  Tire | Size | 195/65R15 91V | 205/55R16 91V | 215/45R17 87W | 215/45R17 91W (reinforced) | Mazda6 MPS: 215/45R18 93Y Except Mazda6 MPS: 215/45R 18 89W
  Air pressure (kPa {(kgf/cm2, bar), <psi>}) | Front | Up to 4 persons | 220 {(2.2, 2.2), <32>} | 2WD: 230 {(2.3, 2.3), <33>} 4WD: 250 {(2.5, 2.5), <36>} | Mazda6 MPS: 260 {(2.6, 2.6), <38>} Except Mazda6 MPS: 220 {(2.2, 2.2), <32>}
  Full load | 240 {(2.4, 2.4), <35>} | 2WD: 240 {(2.4, 2.4), <35>} 4WD:250 {(2.5, 2.5), <36>} | Mazda6 MPS: 270 {(2.8, 2.7), <39>} Except Mazda6 MPS: 240 {(2.4, 2.4), <35>}
  Rear | Up to 4 persons | 220 {(2.2, 2.2), <32>} | 2WD: 230 {(2.3, 2.3), <33>} 4WD: 250 {(2.5, 2.5), <36>} | Mazda6 MPS: 260 {(2.6, 2.6), <38>} Except Mazda6 MPS: 220 {(2.2, 2.2), <32>}
  Full load | 300 {(3.1, 3.0), <44>} | 270 {(2.8, 2.7), <39>} | Mazda6 MPS: 290 {(2.9, 2.9), <42>} Except Mazda6 MPS: 270 {(2.8, 2.7), <39>}
  Remaining tread | (mm {in}) | 1.6 {0.06}
  Wheel and tire | Wheel and tire runout | Radial direction | 1.5 {0.06} max.
  (mm {in}) | Lateral direction | 2.5 {0.10} max. | 2.0 {0.08} max.
  Wheel imbalance | (g {oz}) | Knock-type*2: 9 {0.32} max. | Adhesive-type*1: 13 {0.46} max. Knock-type*2: 8 {0.28} max. | Adhesive-type*1: 11 {0.39} max. Knock-type*2: 7 {0.25} max. | Adhesive-type*1: 10 {0.35} max. Knock-type*2: 6 {0.21} max.
  Temporary spare tire
  Wheel | Size | 15 × 4T | 17 × 4T
  Offset | (mm {in}) | 40 {1.57}
  Pitch circle diameter | (mm {in}) | 114.3 {4.50}
  Material | Steel
  Tire | Size | T115/70 D15 | 2WD: T115/70 D15 4WD: T135/90 D15 | Mazda6 MPS: T145/70 D17 Except Mazda6 MPS: T125/70 D17
  Air pressure | (kPa {(kgf/cm2, bar), <psi>}) | 420 {(4.2, 4.2), <60>}
  Wheel and tire | Wheel and tire runout | Radial direction | 2.0 {0.08} max.
  (mm {in}) | Lateral direction | 2.5 {0.10} max.

  *1 :
Total weight exceeds 160 g {5.65 oz} .
  *2 :
One balance weight: 60 g {2.12 oz} max. If the total weight exceeds 100 g {3.53 oz} on one side, rebalance after moving the tire around on the rim. Do not use three or more balance weights.
  Australian specs

  Item | Specification
  --- | ---
  Standard tire and wheel
  Wheel | Size | 15 × 6J | 16 × 7J | 17 × 7J | 18 × 7J
  Offset | (mm {in}) | 50 {1.97} | 55 {2.17}
  Pitch circle diameter | (mm {in}) | 114.3 {4.50}
  Material | Steel | Aluminum alloy
  Tire | Size | 195/65R15 91V | 205/55R16 91V | 215/45R17 87W | 215/45R18 89W
  Air pressure (kPa {bar} <psi>) | Front | 220 {2.2} <32> | L3 ATX: 230 {2.3} <33> | 260 {(2.6), <38>}
  Rear
  Remaining tread | (mm {in}) | 1.6 {0.06}
  Wheel and tire | Wheel and tire runout | Radial direction | 1.5 {0.06} max.
  (mm {in}) | Lateral direction | 2.5 {0.10} max. | 2.0 {0.08} max.
  Wheel imbalance | (g {oz}) | Knock-type*2: 9 {0.32} max. | Adhesive-type*1: 13 {0.46} max. Knock-type*2: 8 {0.28} max. | Adhesive-type*1: 11 {0.39} max. Knock-type*2: 7 {0.25} max. | Adhesive-type*1: 10 {0.35} max. Knock-type*2: 6 {0.21} max.
  Temporary spare tire
  Wheel | Size | - | 17 × 4T
  Offset | (mm {in}) | - | 40 {1.57}
  Pitch circle diameter | (mm {in}) | - | 114.3 {4.50}
  Material | - | Steel
  Tire | Size | - | T145/70 D17
  Air pressure | (kPa {bar} <psi>) | - | 420 {4.2} <60>
  Wheel and tire | Wheel and tire runout | Radial direction | - | 2.0 {0.08} max.
  (mm {in}) | Lateral direction | - | 2.5 {0.10} max.

  *1 :
Total weight exceeds 160 g {5.65 oz} .
  *2 :
One balance weight: 60 g {2.12 oz} max. If the total weight exceeds 100 g {3.53 oz} on one side, rebalance after moving the tire around on the rim. Do not use three or more balance weights.
  General (L.H.D. R.H.D.) specs

  Item | Specification
  --- | ---
  Standard tire and wheel
  Wheel | Size | 15 × 6J | 16 × 7J | 17 × 7J
  Offset | (mm {in}) | 50 {1.97} | 55 {2.17}
  Pitch circle diameter | (mm {in}) | 114.3 {4.50}
  Material | Steel | Aluminum alloy
  Tire | Size | 195/65R15 91V | 205/55R16 91V | 215/45R17 87W | 215/45R17 91W (reinforced)
  Air pressure (kPa {(kgf/cm2, bar), <psi>}) | Front | Up to 4 persons | 220 {(2.2, 2.2), <32>}
  Full load | 240 {(2.4, 2.4), <35>}
  Rear | Up to 4 persons | 220 {(2.2, 2.2), <32>}
  Full load | 300 {(3.1, 3.0), <44>} | 270 {(2.8, 2.7), <39>}
  Remaining tread | (mm {in}) | 1.6 {0.06}
  Wheel and tire | Wheel and tire runout | Radial direction | 1.5 {0.06} max.
  (mm {in}) | Lateral direction | 2.5 {0.10} max. | 2.0 {0.08} max.
  Wheel imbalance | (g {oz}) | Knock-type*2: 9 {0.32} max. | Adhesive-type*1: 13 {0.46} max. Knock-type*2: 8 {0.28} max. | Adhesive-type*1: 11 {0.39} max. Knock-type*2: 7 {0.25} max.
  Temporary spare tire (General (L.H.D.) specs.)
  Wheel | Size | 15 × 4T
  Offset | (mm {in}) | 40 {1.57}
  Pitch circle diameter | (mm {in}) | 114.3 {4.50}
  Material | Steel
  Tire | Size | T115/70 D15
  Air pressure | (kPa {(kgf/cm2, bar), <psi>}) | 420 {(4.2, 4.2), <60>}
  Wheel and tire | Wheel and tire runout | Radial direction | 2.0 {0.08} max.
  (mm {in}) | Lateral direction | 2.5 {0.10} max.

  *1 :
Total weight exceeds 160 g {5.65 oz} .
  *2 :
One balance weight: 60 g {2.12 oz} max. If the total weight exceeds 100 g {3.53 oz} on one side, rebalance after moving the tire around on the rim. Do not use three or more balance weights.