#
VACUUM PUMP REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

id0411008036e1

1. Remove the battery and battery tray. (See BATTERY REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Remove the air cleaner. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. Remove the vacuum pipe.

4. Remove the nut and bolt shown in the figure, and move the air pipe.

5. Remove the VBC solenoid valve.

6. Remove the nut shown in the figure, and move the fuel pipe.

7. Remove in the order indicated in the table.

1 | Vacuum hose
2 | Bolt
3 | Vacuum pump (See Vacuum Pump Installation Note)
4 | O-ring

8. Install in the reverse order of removal.

## Vacuum Pump Installation Note

1. Be careful the O-ring is not pinched when installing the vacuum pump.