#
WINDSHIELD INSTALLATION

id091200417900

  Caution

  • To prevent the sealant from cracking or the glass from being pushed out by air pressure if a door is closed, open all of the windows and leave them open until the sealant has hardened.

1. Cut away the old sealant using a razor so that 1-2 mm {0.04-0.07 in} thickness of sealant remains around the circumference of the frame.

  Warning

  • Using a razor with bare hands can cause injury. Always wear gloves when using a razor.

2. If the sealant has come off completely in any one place, apply some primer after degreasing, and allow it approx. 30 min to dry. Then put on new sealant to create a 2 mm {0.08 in} layer.

3. Clean and degrease an approx. 50.0 mm {1.97 in} wide strip around the circumference of the glass and the bonding area on the body.

4. If installing reused glass, install pins at the ceramic void on the upper part of the windshield.

5. If installing reused glass, align the front windshield molding marking and the center of the upper section of the windshield, then install the molding to the windshield.

6. Use only glass primer on the glass, and body primer on the body and the molding. Allow it to dry for approx. 30 min.

  Caution

  • Keep the area free of dirt and grease, and do not touch the surface or the primer may not properly bond to the surface of the glass and body, which may cause leaks to occur.

7. Apply urethane to the area of the glass surface as shown in the figure.

8. Set the windshield in place and insert the pins into the body. Install the windshield.

9. Verify that the gap of the A pillar part as shown the figure.

10. Keeping the measurement of the molding lip gap within specification, press completely along the perimeter of the glass.

11. Install the seaming welt.

12. Install the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

13. Install the headliner. (See HEADLINER REMOVAL/INSTALLATION [4SD, 5HB].) (See HEADLINER REMOVAL/INSTALLATION [WGN].)

14. Install the rearview mirror. (See REARVIEW MIRROR REMOVAL/INSTALLATION.)

15. Allow the sealant to harden completely.

  Sealant hardening time: 24 h