#
AUTO LEVELING CONTROL MODULE FUNCTION

id091800103900
• In order to prevent the blinding of oncoming traffic and improve visibility, the auto leveling control modules automatically control the optical axis direction for optimal illumination based on signal inputted from the ABS (DSC) HU/CM and the auto leveling sensor.
• With an on-diagnostic function included for auto leveling control module, servicing based on display of DTCs using the SST (WDS or equivalent) has been improved.