#
KOEO/KOER SELF TEST [MZR-CD (RF Turbo)]

id0102f1801200

  Note

  • Warm up until the exhaust gas temperature (EXHTEMP1, EXHTEMP2, EXHTEMP3 PID) is 100 °C {212 °F} or more before performing "KOER SELF TEST".

1. Perform the necessary vehicle preparation and visual inspection.

2. Connect the WDS or equivalent to the vehicle DLC-2 16-pin connector located in the driver compartment.

3. Retrieve the KOEO/KOER DTCs using the WDS or equivalent.