#
NO.1 NO SOUND OF THE CASSETTE TAPE

id0903a1870400

1 | No sound of the cassette tape./00:Er01, 00:Er03, 00:Er10
TROUBLESHOOTING HINTS • Tape head gathers oxide residue from cassette tape. • Cassette tape player is malfunctioning.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Replace with the cassette tape known to be good. • Does the cassette tape player sound? | Yes | The cassette tape player is normal. Explain to the customer that the cassette tape is malfunctioning.
No | Go to the next step.
2 | • Clean the tape head using the good quality head-cleaning tape. • Does the cassette tape player sound? | Yes | Explain the repairs (head cleaning) to the customer.
No | Replace the cassette tape player.