#
REAR DOOR TRIM REMOVAL/INSTALLATION

id091700460000

1. Disconnect the negative battery cable if equipped with power window system.

2. Remove the regulator handle if equipped.

3. Open the cap using a small screwdriver, then remove the screw.

4. Remove the inner handle cover.

5. Remove the cover, then remove screws.

6. Disengage clips A from the rear door using a fastener remover.

7. Pull the rear door trim upward, then disengage tabs B from the rear door.

8. Disconnect the power window subswitch connector.

9. Remove the rear door trim.

10. Remove the switch panel from the rear door trim.

11. Install in the reverse order of removal.