#
PID/DATA MONITOR TABLE [DISCHARGE HEADLIGHT]

id0902b2862100

## LHID

PID Name (Definition) | Unit/Condition | Condition/Specification | Discharge headlight control module (LH) terminal
--- | --- | --- | ---
CCNT (Number of continuous codes) | - | • DTC is detected: 1-255 • DTC is not detected: 0 | -
ONDEMDTC (Number of on-demand codes) | - | • DTC is detected: 1-255 • DTC is not detected: 0 | -
L_VOLT_L (Discharge headlight control (LH) input voltage) | VOLTAGE | Headlight switch at ON: B+ | D
GDL_P_L (Output power to discharge headlight bulb (LH)) | WATT | Headlight switch at ON: 35-65 W | -
GDL_V_L (Output voltage to discharge headlight bulb (LH)) | VOLTAGE | Headlight switch at ON: 68-112 V | -

## RHID

PID Name (Definition) | Unit/Condition | Condition/Specification | Discharge headlight control module (RH) terminal
--- | --- | --- | ---
CCNT (Number of continuous codes) | - | • DTC is detected: 1-255 • DTC is not detected: 0 | -
ONDEMDTC (Number of on-demand codes) | - | • DTC is detected: 1-255 • DTC is not detected: 0 | -
L_VOLT_R (Discharge headlight control module (RH) input voltage) | VOLTAGE | Headlight switch at ON: B+ | D
GDL_P_R (Output power to discharge headlight bulb (RH)) | WATT | Headlight switch at ON: 35-65 W | -
GDL_V_R (Output voltage to discharge headlight bulb (RH)) | VOLTAGE | Headlight switch at ON: 68-112 V | -