#
POWER DOOR LOCK SYSTEM CONSTRUCTION/OPERATION

id0914b3104600
• Consists of the following parts;

  - BCM
  - Front door lock actuator
  - Rear door lock actuator
  - Trunk lid opener/liftgate lock actuator
  - Door lock-link switch (built into the driver-side front door lock actuator)
  - Door key cylinder switch (built into the driver-side front door lock actuator)

• Unlocking/locking of all doors and liftgate is performed by operation of the door key cylinder (door key cylinder switch) and driver-side door knob (door lock-link switch).
• When unlocking using the door key cylinder, operating one time will unlock the driver-side door and operating a second time will unlock the passenger-side door.
• When any door is open, locking operation using the door key cylinder or the driver-side door lock knob is cancelled and the doors are unlocked. (Lock cancel function)

1 | Door switch (door open or closed)
2 | • Trunk compartment light switch (4SD) • Liftgate latch switch (5HB, WGN) (trunk lid/liftgate open or closed)
3 | Door key cylinder switch (lock or unlock)
4 | Door lock-link switch (lock or unlock)
5 | Front door lock actuator
6 | Rear door lock actuator
7 | • Trunk lid opener (4SD) • Liftgate lock actuator (5HB, WGN)