#
COOLING FAN MOTOR INSPECTION [L8, LF, L3]

id0112b28018b1

  Note

  • There are three types of cooling fan components, A, B, and C. Types A, B, and C can be identified from the number of blades on the cooling fans No. 1 and No. 2. Refer to the following table to identify the cooling fan type.

Cooling fan components | Number of blades
--- | ---
Cooling fan No.1 (LH) | Cooling fan No.2 (RH)
Type A | 5 | 7
Type B | 7 | 5
Type C | 7 | 4

1. Verify that the battery is fully charged. (See BATTERY INSPECTION [L8, LF, L3, L3 Turbo].)

2. Disconnect the cooling fan motor connector.

3. Install a tester and battery to the cooling fan motor connector as shown in the figure.

4. Verify that fan motor operates smoothly at the standard current.

  • If not within the specification, replace the fan motor.

Cooling fan motor current [Type A]

  No.1: 5.5-7.5 A
  No.2: 5.5-7.5 A

Cooling fan motor current [Type B]

  No.1: 8.5-11.5 A
  No.2: 8.5-11.5 A

Cooling fan motor current [Type C]

  No.1: 4.4-7.4 A
  No.2: 6.5-9.5 A