#
TCM REMOVAL/INSTALLATION [JA5AX-EL]

id051705800400

1. Disconnect the negative battery cable.

2. For R.H.D., perform the following procedures.

  (1) Remove the front side trim (left-side).
  (2) Partially peel back the flower covering.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

U.K. specs.

.

1 | Control unit bracket (See Set Nut/bolt Removal Note.) (See Set Nut/bolt Installation Note.)
2 | TCM connector
3 | TCM

European (L.H.D.) specs.

.

1 | 4WD control module connector
2 | TCM connector
3 | 4WD control module
4 | TCM

## Set Nut/bolt Removal Note

1. Using a chisel and hammer, cut a groove on the head of the set nut/bolt so that a screwdriver can be inserted.

2. Loose the set nut/bolt using an impact screwdriver or pliers.

## Set Nut/bolt Installation Note

1. Install a new set nut/bolt and tighten it until the neck of the nut/bolt is cut.