#
POWER STEERING OIL PUMP REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

id0614008007c4

1. Remove the battery and battery tray. (See BATTERY REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Remove the air cleaner. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. Remove the vacuum pipe.

4. Remove the air pipe and the air hose. (turbocharger-charge air cooler) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

5. Remove the air pipe and the air hose. (Air cleaner cover-turbocharger) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

.

1 | Pressure switch connector
2 | Pressure pipe
3 | Return hose
4 | Power steering oil pump
5 | O-ring