#
NO.1 CD PLAYER/CHANGER DOES NOT LOAD THE CD OR EJECTS THE CD IMMEDIATELY.

id0903a1826100

1 | CD player/changer does not load the CD or ejects the CD immediately./03:Er01, 03:Er10, 06:Er01, 06:Er10, 10:Er01, 10:Er10, 22:Er01, 22:Er10
TROUBLESHOOTING HINTS • CD is inserted upside down. • Audio units is malfunctioning. • Defective CD. (e.g., cracked, badly bent, rough edges, scratch, dirty CD, condensation). • Non-conventional discs. (e.g., 8cm (3 in) CD, 8cm (3 in) disc adapter, heart-shaped disc, octagonal disc) • Poor connection of audio unit connector or terminal. (e.g., damaged, bent, pulled-out pin, corrosion) • Deformed disc is used. (e.g., out of specification (thickness), bent disc)

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Is CD inserted properly, label-side up? | Yes | Go to the next step.
No | Explain to the customer that CD should be inserted into the slot, label-side up.
2 | • Replace with a CD player/changer load the CD? • Does the CD player/changer load the CD? | Yes | Go to the next step.
No | Replace the audio unit.
3 | Visually inspect the CD. - Is there any dirt, scratch or deformation on the CD? - Is the CD a non-conventional disc? | Yes | Explain to the customer that the defective CD or non-conventional disc cannot be use.
No | Go to the next step.
4 | • Turn the ignition switch to the LOCK position. • Inspect the connection of the audio unit connector (24-pin). • Inspect both audio unit connector and wiring harness-side connector for poor connection (such as damaged/bent/pulled-out pins, corrosion) • All the pins and connector normal? | Yes | Replace the audio unit.
No | if the audio unit connector/pin is wrong: Replace the audio unit. If the wiring harness-side connector/pin is wrong: Repair or replace the pins and/or the connector.