#
DTC P2119 [L3 Turbo]

id0102b7811600

DTC P2119 | Throttle actuator control throttle body range/performance problem
--- | ---
DETECTION CONDITION | • The PCM compares the TP with the default TP when the ignition switch is off. If the TP is higher than the default TP, the PCM determines that there is a throttle actuator control throttle body range/performance problem. Diagnostic support note • This is a continuous monitor (CCM). • The MIL illuminates if the PCM detects the above malfunctioning condition in the first drive cycles. • FREEZE FRAME DATA is available. • DTCs are stored in the PCM memory.
POSSIBLE CAUSE | • Throttle actuator malfunction • Throttle valve malfunction • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA AND DIAGNOSTIC MONITORING TEST RESULTS HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service information. If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT THROTTLE ACTUATOR • Inspect the throttle actuator. (See Resistance Inspection.) • Is there any malfunction? | Yes | Replace the throttle body, then go to Step 5. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo], INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)
No | Go to the next step.
4 | INSPECT TP SENSOR • Inspect the TP sensor. (See THROTTLE POSITION (TP) SENSOR INSPECTION [L3 Turbo].) • Is there any malfunction? | Yes | Replace the TP sensor, then go to the next step. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo], INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)
No | Go to the next step.
5 | VERIFY TROUBLESHOOTING OF DTC P2119 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Turn the ignition switch to the ON position (Engine off), then off. • Is the PENDING CODE for this DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [L3 Turbo].)
No | Go to the next step.
6 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [L3 Turbo].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [L3 Turbo].)
No | DTC troubleshooting completed.