#
DTC P2456 [MZR-CD (RF Turbo)]

id0102f1118700

DTC P2456 | Exhaust gas pressure sensor circuit intermittent/erratic
--- | ---
DETECTION CONDITION | • The PCM monitors the input signal from the exhaust gas pressure sensor. If the differential pressure between the maximum and minimum value of the exhaust gas pressure sensor is less than 90 Pa {0.68 mmHg, 0.027 inHg}, the PCM determines that there is a malfunction in the exhaust gas pressure sensor.
POSSIBLE CAUSE | • Exhaust gas pressure sensor malfunction • Connector or terminal malfunction • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY CURRENT SIGNAL STATUS: IS CONCERN INTERMITTENT OR CONSTANT? • Connect the WDS or equivalent to the DLC-2. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the PENDING CODE for this DTC present? | Yes | Go to the next step.
No | Intermittent concern exists. Perform the "INTERMITTENT CONCERN TROUBLESHOOTING". (See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
4 | INSPECT EXHAUST GAS PRESSURE SENSOR CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Disconnect the exhaust gas pressure sensor connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 7.
No | Go to the next step.
5 | INSPECT EXHAUST GAS PRESSURE SENSOR • Inspect the exhaust gas pressure sensor. (See EXHAUST GAS PRESSURE SENSOR INSPECTION [MZR-CD (RF Turbo)].) • Is there any malfunction? | Yes | Replace the exhaust gas pressure sensor, then go to Step 7. (See EXHAUST GAS PRESSURE SENSOR/EXHAUST GAS PRESSURE CORRECTION TEMPERATURE SENSOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
6 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the engine switch off. • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to the next step.
No | Go to the next step.
7 | VERIFY TROUBLESHOOTING OF DTC P2456 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the PENDING CODE for this DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
8 | VERIFY AFTER REPAIR PROCEDURE • Perform the Repair Verification Drive Mode. (See OBD DRIVE MODE [MZR-CD (RF Turbo)].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | DTC troubleshooting completed.