#
FRONT BUMPER REINFORCEMENT REMOVAL/INSTALLATION

id091000405400

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove the headlight. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

4. Support the radiator and the condenser using the wire.

5. Remove the bolt.

6. Remove the front bumper reinforcement.

7. Install in the reverse order of removal.