#
DIFFERENTIAL OIL TEMPERATURE SENSOR REMOVAL/INSTALLATION [L3 Turbo]

id0318a2805700

  Warning

  • Hot differential oil may cause severe burns. Do not perform maintenance while differential oil is hot.

1. Disconnect the negative battery cable.

2. Disconnect the differential oil temperature sensor connector.

3. Remove the differential oil temperature sensor.

4. Apply differential oil to the O-ring.

5. Install the differential oil temperature sensor.

Tightening torque

  12.7-17.3 N·m {1.3-1.7 kgf·m, 9.4-12.7 ft·lbf}

6. Connect the differential oil temperature sensor connector.

7. Connect the negative battery cable.