#
SHIFT INTERLOCK MECHANISM OPERATION [A26M-R, A26MX-R]

id0515a8101400
• During shifting, the shift forks and control rod, except for the one in operation, are locked in the neutral position by the interlock plate.

1 | Reverse shift fork
2 | Inner lever
3 | 5th/6th shift fork
4 | Interlock plate
5 | 1st/2nd shift fork
6 | 3rd/4th control rod
7 | Neutral
8 | 1st
9 | 2nd
10 | 3rd
11 | 4th
12 | 5th
13 | 6th
14 | Reverse