#
TRANSFER OIL INSPECTION [JA5AX-EL]

id031611800200

1. Park the vehicle on level ground.

2. Remove the PTO heat shield.

3. Remove the filler plug.

4. Verify that the oil is near the brim of the plug port.

  • If the oil level is low, add the specified amount and type of oil through the filler plug hole.

Transfer oil [JA5AX-EL]

  Specified oil grade: API Service GL-5
  Specified oil viscosity: SAE 80W-90

5. Apply a sealant to the thread area of filler plug.

Specified sealant

  TB1215 or equivalent

6. Install the filler plug.

Tightening torque

  9.8-19.6 N·m
  {100-199 kgf·cm, 116-175 in·lbf}

7. Install the PTO heat shield. (See PTO Heat Shield Installation Note.)