#
EXTERIOR OPEN/CLOSE FUNCTION OPERATION

id091200102300
• With the function, all door glass can open/close in conjunction with the UNLOCK/LOCK operation of the transmitter, and request switch (with advanced keyless system).
• One opening operation fully opens (automatic open) all door glass, and close operation operates only when the operation (manual close) is being performed.
• During IG OFF timer operation (power window system operates approx. 40 s after IG OFF), the power window switch operation has priority over the exterior open/close function.
• Auto reverse pinch protection operation has priority when the door glass is obstructed during close operation.
• The BCM sends the signal requiring the open/close operation to the power window control module (power window main switch) based on the signals input from the switches.
• The power window control module (power window main switch) sends open/close operation signal to the power window motor based on the required signal, and operates the door glass.

## Open Function/Operation in Conjunction with Transmitter

• The door glass can be opened by holding the button in the UNLOCK position for approx. 1.5 s or more within the transmitter reception area.
• When the door glass is not fully open, operate and hold the transmitter UNLOCK position for approx. 1.5 s, and the door glass performs automatic open operation to fully open the door glass. During the automatic open operation, if the transmitter is operated again*1, it stops in that position.
  *1 :
The operation button can be either the LOCK/UNLOCK/PANIC button. Also, the holding time is not factored.

.

1 | Close operation
2 | Open operation
3 | Close (lock button hold approx. 1.5 s)
4 | Lock signal
5 | Close request signal
6 | Power window switch
7 | Close operation signal
8 | Open (unlock button hold approx. 1.5 s)
9 | Unlock signal
10 | Open request signal
11 | Open operation signal

## Close Function/Operation in Conjunction with Request Switch

• If the driver-side request switch is operated and held for approx. 1.5 s or more while the card key (transmitter) is within the reception area and the door glass is open, the door glass performs manual close operation. When the switch is released, the operation stops.
• During the operation, when the open/close function in conjunction with the key operation is performed, or the open/close function in conjunction with the transmitter is performed, these functions have priority over the operation.

1 | Close operation
2 | Request switch (driver's side)
3 | Close (lock, hold approx. 1.5 s)
4 | Lock signal
5 | Keyless control module
6 | Close request signal
7 | Power window switch
8 | Close operation signal

## Operation Prohibition/Stop Condition

• When the following conditions are met before the operation, the exterior open/close function does not operate. Also, if the conditions are met during the operation, the operation stops.

  - Either door is open (when the door switch is ON)
  - The key is inserted in the steering lock (when the key reminder is ON)
  - The push switch is pressed in or the start knob (ignition switch) is in a position other than the LOCK (with advanced keyless system)
  - The transmitter is not in the reception area
  - The card key (transmitter) is not in the reception area when the driver-side request switch is operated (with advanced keyless system)
  - The transmitter is operated during the operation (LOCK, UNLOCK, PANIC operation)