#
AUTO LEVELING CONTROL MODULE CONFIGURATION

id091800895500

1. Connect the SST (WDS or equivalent) to the DLC-2.

2. Input vehicle information following the directions on the screen.

3. Select "Module programming".

4. Select "Programmable module installation".

5. When performing configuration corresponding to each auto leveling control unit, select the following items and perform procedures according to directions on the screen.

Items

  • Main: "LHID"
  • Sub: "RHID"

6. Retrieve DTCs by the WDS or equivalent, then verify that there is no DTC present.

  • If DTC is present, perform applicable DTC inspection.