#
NO. 7 ALL DOOR GLASSES OPERATE ACCIDENTALLY

id090397822300

7 | All door glasses operate accidentally
POSSIBLE CAUSE | • Transmitter malfunction • Request switch malfunction • Open or short circuit in wiring harness between request switch (each door) and keyless control module. • Power window main switch malfunction • Power window subswitch malfunction • Open or short circuit in wiring harness between power window main switch and power window subswitch • BCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Inspect if malfunction is in operating by transmitter | Yes | Inspect the transmitter.
No | With keyless entry system • Go to Step 3. With advanced keyless system • Go to the next step.
2 | • Inspect if malfunction is in operating by request switch | Yes | Inspect the following parts and repair or replace. • Request switch (See REQUEST SWITCH INSPECTION.) • Wiring harness between request switch and keyless control module
No | Go to the next step.
3 | • Inspect if malfunction is in operating power window main switch | Yes | Inspect power window main switch (See POWER WINDOW MAIN SWITCH INSPECTION.)
No | Go to the next step.
4 | • Inspect if malfunction is in without operating Step1to 3 | Yes | Inspect the following parts and repair or replace • Power window subswitch (See POWER WINDOW SUBSWITCH INSPECTION.) • BCM (See BODY CONTROL MODULE (BCM) INSPECTION.) • Wiring harness between power window subswitch and power window main switch
No | Reinspect for malfunction recurrence.If the malfunction is not corrected, repeat the procedure from Step 1.