#
CAR-NAVIGATION SYSTEM OUTLINE

id092000100800
• A 7 inch wide, pop-up LCD (*TFT) has been adopted to improve marketability.
• A hybrid in car-navigation system and map-matching function has been adopted to improve accuracy of vehicle position.
• A voice recognition function has been adopted.
• A remote control with an infrared transmitter has been adopted to improve operational ability. (U.K. specs. only)
• The languages and voices available for use with the car-navigation unit include English (U.S.A), English (U.K.), French, German, Dutch, Spanish, Portuguese, Swedish, Danish, Norwegian, Finnish, and Italian. However, the language used in this manual is in English only.
  *TFT :
Thin Film Transistor

## Specifications

### Car-navigation unit

Item | Specification
--- | ---
Unit type | Stand alone
Rated voltage | (V) | 12
ROM type | DVD-ROM
Output impedance | (ohm) | Standard: 4, BOSE: 4.7
Voice guidance output power | (W) | 5

### LCD unit

Item | Specification
--- | ---
Unit type | Pop-up
Rated voltage | (V) | 12
Display (for car-navigation system) | Size | (inch) | 7 (wide)
Type | TFT (Thin Film Transistor); Full-color
Display (for audio, DIS and A/C) | Type | LCD; Amber-color

### Speaker

  • Refer to audio system. (See Specifications.)