#
BAROMETRIC PRESSURE (BARO) SENSOR INSPECTION [MZR-CD (RF Turbo)]

id0140f1818700

  Note

  • Perform the following inspection only when directed.
  • The following vacuum values are indicated by relative pressure from the PCM. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

1. Connect the WDS or equivalent to the DLC-2.

2. Turn the engine switch to ON.

3. Select BARO on the WDS or equivalent.

4. Verify that the BARO PID (pressure) and barometric pressure are practically equal.

  • If not as verified, perform the "Circuit Open/Short Inspection".

  - If there is no open or short circuit, replace the PCM. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)