#
ENGINE COOLANT PROTECTION INSPECTION [L8, LF, L3, L3 Turbo]

id0112b2800400

1. Measure the engine coolant temperature and specific gravity using a thermometer and a hydrometer.

  Caution

  • Use engine coolant at a concentration that meets the environmental conditions in which the vehicle is driven, otherwise engine damage could occur.
  • The engine has aluminum parts and must be protected by an ethylene-glycol-based coolant to prevent corrosion and freezing.
  • Do not use coolants containing Alcohol, Methanol, Borate or Silicate. These coolants could damage the cooling system.
  • Use only soft (demineralized) water in the coolant mixture. Water that contains minerals will cut down on the coolant's effectiveness.
  • Engine coolant damages paint. If engine coolant does get on a painted surface, rinse it off quickly.

  Note

  • If the "FL22" mark is shown on or near the cooling system cap, use FL22 type engine coolant.
  • FL22 type engine coolant is shipped as a diluted solution (55% coolant, 45% water). Use the solution as is when replacing coolant.

2. Determine the engine coolant protection level by referring to the graph shown.

  • If the engine coolant protection level is not correct, add water or engine coolant.