#
BRAKES SPECIFICATIONS

id040000100300

European (L.H.D. U.K.) specs.

Item | Specification
--- | ---
Brake pedal | Type | Suspended
Pedal lever ratio | 2.7
Max. stroke | (mm {in}) | 128.5 {5.06}
Master cylinder | Type | Tandem (with level sensor)
Cylinder diameter | (mm {in}) | 20.64 {0.813}
Front disc brake | Type | Ventilated disc
Cylinder bore | (mm {in}) | L8, LF, L3 (except 18 inch wheel), MZR-CD (RF Turbo): 57.15 {2.250} L3 (18 inch wheel), L3 Turbo: 57 {2.2}
Pad dimensions (area × thickness) | L8 (4SD, 5HB): 4,220 {6.75} × 10.0 {0.39} L8 (WGN), LF, L3 (except 18 inch wheel), MZR-CD (RF Turbo): 4,010 {6.42} × 12.0 {0.47} L3 (18 inch wheel), L3 Turbo: 3,918 {6.27} × 12.5 {0.49}
(mm2 {in2} × mm {in})
Disc plate dimensions (outer diameter × thickness) | L8 (4SD, 5HB): 274 {10.8} × 24.0 {0.945} L8 (WGN), LF, L3 (except 18 inch wheel), MZR-CD (RF Turbo): 283 {11.1} × 25.0 {0.984} L3 (18 inch wheel), L3 Turbo: 320 {12.6} × 25.0 {0.984}
(mm {in} × mm {in})
Rear brake (disc) | Type | Solid disc
Cylinder bore | (mm {in}) | L8, LF, L3 (except 18 inch wheel), MZR-CD (RF Turbo): 34.93 {1.375} L3 (18 inch wheel), L3 Turbo: 33.96 {1.337}
Pad dimensions (area × thickness) | L8, LF, L3 (except 18 inch wheel), MZR-CD (RF Turbo): 2,820 {4.51} × 8.0 {0.31} L3 (18 inch wheel), L3 Turbo: 2,195 {3.51} × 9.0 {0.35}
(mm2 {in2} × mm {in})
Disc plate dimensions (outer diameter × thickness) | L8, LF, L3 (except 18 inch wheel), MZR-CD (RF Turbo): 280 {11.0} × 10.0 {0.39} L3 (18 inch wheel), L3 Turbo: 314 {12.4} × 11.0 {0.43}
(mm {in})
Power brake unit | Type | Vacuum multiplier, single diaphragm
Diameter | (mm {in}) | 276.1 {10.87}
Braking force control device | Type | EBD (Electronic Brakeforce Distribution)
Parking brake | Type | Mechanical two-rear-wheel control
Operation system | Center lever type
Brake fluid | Type | SAE J1703, FMVSS 116 DOT-3 or DOT-4

Australian, General (L.H.D. R.H.D.) specs.

Item | Specification
--- | ---
Brake pedal | Type | Suspended
Pedal lever ratio | 2.7
Max. stroke | (mm {in}) | 128.5 {5.06}
Master cylinder | Type | Tandem (with level sensor)
Cylinder diameter | (mm {in}) | 20.64 {0.813}
Front disc brake | Type | Ventilated disc
Cylinder bore | (mm {in}) | Except L3 Turbo: 57.15 {2.250} L3 Turbo: 57 {2.2}
Pad dimensions (area × thickness) | 4SD (except L3 Turbo), 5HB, WGN (except Australian specs.): 4,220 {6.75} × 10.0 {0.39} WGN (Australian specs.): 4,010 {6.42} × 12.0 {0.47} 4SD (L3 Turbo): 3,918 {6.27} × 12.5 {0.49}
(mm2 {in2} × mm {in})
Disc plate dimensions (outer diameter × thickness) | 4SD (except L3 Turbo), 5HB, WGN (except Australian specs.): 274 {10.8} × 24.0 {0.945} WGN (Australian specs.): 283 {11.1} × 25.0 {0.984} 4SD (L3 Turbo): 320 {12.6} × 25.0 {0.984}
(mm {in} × mm {in})
Rear brake (disc) | Type | Solid disc
Cylinder bore | (mm {in}) | Except L3 Turbo: 34.93 {1.375} L3 Turbo: 33.96 {1.337}
Pad dimensions (area × thickness) | Except L3 Turbo: 2,820 {4.51} × 8.0 {0.31} L3 Turbo: 2,195 {3.51} × 9.0 {0.35}
(mm2 {in2} × mm {in})
Disc plate dimensions (outer diameter × thickness) | Except L3 Turbo: 280 {11.0} × 10.0 {0.39} L3 Turbo: 314 {12.4} × 11.0 {0.43}
(mm {in})
Power brake unit | Type | Vacuum multiplier, single diaphragm
Diameter | (mm {in}) | 276.1 {10.87}
Braking force control device | Type | Without ABS (ABS/TCS) or DSC: Dual proportioning valve With ABS (ABS/TCS) or DSC: EBD (Electronic Brakeforce Distribution)
Parking brake | Type | Mechanical two-rear-wheel control
Operation system | Center lever type
Brake fluid | Type | SAE J1703, FMVSS 116 DOT-3