#
INTAKE SHUTTER VALVE POSITION SENSOR INSPECTION [MZR-CD (RF Turbo)]

id0140f1445800

  Note

  • Perform the following test only when directed.

## Voltage Inspection

1. Turn the engine switch to ON.

2. Monitor the TP PID using the WDS or equivalent.

  • If not as specified, perform the "Circuit Open/Short Inspection".

  - If there is no open/short circuit, replace the intake shutter valve. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)])

TP1 PID

  Approx. 4.2 V

3. Start the engine and warm up the engine completely.

4. Monitor the TP PID using the WDS or equivalent at idle.

  • If not as specified, perform the "Circuit Open/Short Inspection".

  - If there is no open/short circuit, replace the intake shutter valve. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)])

TP1 PID

  0.75-3.79 V

## Circuit Open/Short Inspection

1. Disconnect the PCM connector. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)])

2. Disconnect the intake shutter valve connector.

3. Inspect for open/short circuit in the following wiring harnesses.

  • If there is open/short circuit, repair or replace wiring harnesses.

### Open circuit

  • Intake shutter valve terminal C and PCM terminal 70
  • Intake shutter valve terminal E and PCM terminal 45
  • Intake shutter valve terminal F and PCM terminal 86

### Short circuit

  • Intake shutter valve terminal C and power supply
  • Intake shutter valve terminal E and power supply
  • Intake shutter valve terminal E and body ground
  • Intake shutter valve terminal F and power supply
  • Intake shutter valve terminal F and body ground