#
SEAT POSITION MEMORY FUNCTION CONSTRUCTION/OPERATION

id091300200100

## Structural View

.

1 | Position memory switch
2 | Set switch
3 | Memory switch
4 | Slide motor
5 | Rear tilt motor
6 | Front tilt motor
7 | Recliner motor
8 | Power seat switch
9 | Position memory control module
10 | Transmitter (with advanced keyless system)
11 | Transmitter (with keyless entry system)

## System wiring diagram

.

1 | Instrument cluster
2 | Door ajar warning light
3 | Door switch (driver's side)
4 | ABS HU/CM
5 | Keyless control module
6 | Power seat switch
7 | Slide switch
8 | Front tilt switch
9 | Rear tilt switch
10 | Recliner switch
11 | Position memory switch
12 | Set switch
13 | Memory switch 1
14 | Memory switch 2
15 | Memory switch 3
16 | Slide motor
17 | Front tilt motor
18 | Rear tilt motor
19 | Recliner motor
20 | Position sensor (slide motor)
21 | Position sensor (front tilt motor)
22 | Position sensor (rear tilt motor)
23 | Position sensor (recliner motor)
24 | Position memory control module

## Operation

### SEAT POSITION DETECTION FUNCTION

  • Position memory control module detects the motor position (seat position) according to the pulse signal from the position sensors installed to each motor.

### SEAT POSITION MEMORY FUNCTION

  • Three seat positions can be programmed in the position memory control module corresponding to the memory switch.
  • Seat position can be programmed corresponding to each transmitter.
  - Transmitter (advanced keyless system) : 6
  - Transmitter (keyless entry system) : 3
  • Programming of the seat position is possible according to the following procedures.

SEAT POSITION SWITCH

  1. Slide the seat manually to the desired position.
  2. Press the set switch while pressing memory switches 1, 2, or 3.
  3. Buzzer sounds and the seat position is programmed.

TRANSMITTER

  1. Slide the seat manually to the desired position.
  2. Press the UNLOCK button on the transmitter while pressing the set switch.
  3. Buzzer sounds and seat position is programmed.
  Note

  • Memory operation is possible when all of the following three conditions are met.

  - Memory call up operation has not been performed.
  - Manual operation has not been performed.
  - When the vehicle is stopped (vehicle speed 2 km/h [1.24 mph] or less).

  • Memory is reprogrammed when the seat position is added to the memory switch which has already been programmed.
  • If the negative battery cable is disconnected and 5 s or more have elapsed, all of the seat position memory will be erased.

### MEMORY CALL UP FUNCTION (MEMORY SWITCH)

  • Call up operation is performed which slides the seat to the programmed seat position by the memory switch operation.

AUTO CALL UP

  • If the following conditions are met, the seat position is automatically called up by the memory switch operation.
  - Door is open (door switch on).
  - Seat position has been programmed.
  - Memory switch and set switch are off.
  - Ignition switch is in the LOCK position.
  - When the vehicle is stopped (vehicle speed 2 km/h [1.24 mph] or less).
  Note

  • Auto call up continues when the door is closed (door switch off) or the ignition switch is turned to the ON position during the auto call up.
  • Auto call up is cancelled when any of the following conditions are met during the auto call up.

  - Manual operation using the power seat switch has been operated
  - Memory switch or set switch has been operated
  - LOCK/UNLOCK operation has been performed using the transmitter with the ignition switch in the LOCK position.
  - While driving (vehicle speed 2 km/h [1.24 mph] or more).

MANUAL CALL UP

  • When the following conditions are met, the call up operation is performed only while the memory switch is being operated.
  - Door is closed (door switch off) or the ignition switch is in the ON position.
  - Seat position has been programmed.
  - Memory switch and set switch are off.
  - When the vehicle is stopped (vehicle speed 2 km/h [1.24 mph] or less).
  Note

  • Auto call up is cancelled when any of the following conditions are met during the manual call up.

  - Memory switch operation has stopped.
  - Manual operation using the power seat switch has been performed.
  - LOCK/UNLOCK operation has been performed using the transmitter with the ignition switch in the LOCK position.
  - While driving (vehicle speed 2 km/h [1.24 mph] or more).

### MEMORY CALL UP FUNCTION (TRANSMITTER)

  • When the door is opened within approx. 2 s after it is unlocked using the transmitter, the auto call up operation slides the seat to the programmed position.
  • Seat position is automatically called up when the following conditions are met.
  - Door is closed (door switch off).
  - Seat position has been programmed.
  - Ignition switch is in the LOCK position.
  - Memory switch and set switch are off.
  - When the vehicle is stopped (vehicle speed 2 km/h [1.24 mph] or less).
  Note

  • Auto call up continues when the door is closed (door switch off) or the ignition switch is turned to the ON position during the auto call up.
  • Auto call up is cancelled if any of the following conditions are met during the auto call up.

  - Manual operation using the power seat switch has been performed.
  - Memory switch or the set switch has been operated.
  - LOCK/UNLOCK operation using the transmitter has been performed with the ignition switch in the LOCK position.
  - While driving (vehicle speed 2 km/h [1.24 mph] or more)