#
NO.28 FUEL FILLING SHUT OFF ISSUES [L3 Turbo]

id0103b4803400

28 | Fuel filling shut off issues
DESCRIPTION | • Fuel does not shut off properly.
POSSIBLE CAUSE | • Clogged EVAP pipes • Nonreturn valve malfunction • Fuel shut-off valve malfunction • Fuel nozzle malfunction • Fuel nozzle is not inserted correctly. Warning • The following troubleshooting flow chart contains the fuel system diagnosis and repair procedures. Read the following warnings before servicing the fuel system: - Fuel vapor is hazardous. It can easily ignite, causing serious injury and damage. Always keep sparks and flames away from fuel. - Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Fuel can also irritate skin and eyes. To prevent this, always complete "BEFORE REPAIR PROCEDURE" and "AFTER REPAIR PROCEDURE" described in this manual. (See BEFORE SERVICE PRECAUTION [L3 Turbo].) (See AFTER SERVICE PRECAUTION [L3 Turbo].) Caution • Disconnecting/connecting the quick release connector without cleaning it may possibly cause damage to the fuel pipe and quick release connector. Always clean the quick release connector joint area before disconnecting/connecting, and make sure that it is free of foreign material.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Connect the WDS or equivalent to the DLC-2. Turn the ignition switch to the ON position (Engine off). Retrieve any DTCs. Are there any DTCs displayed? | Yes | DTC is displayed: Go to the appropriate DTC test.
No | No DTC is displayed: Go to the next step.
2 | Remove the fuel-filler pipe. Make sure nonreturn valve is installed properly. Inspect the nonreturn valve operation. Is nonreturn valve normal? | Yes | Inspect for the following: • Improper use of fuel nozzle • Fuel is not inserted correctly. • Inspect fuel shut-off valve.
No | Nonreturn valve is installed improperly: • Reinstall the nonreturn valve to proper position. Nonreturn valve does not operate properly: • Replace the nonreturn valve.
3 | Verify test results. • If normal, return to the diagnostic index to service any additional symptoms. • If a malfunction remains, inspect the related Service Bulletins and/or On-line Repair Information and perform the repair or diagnosis. - If the vehicle is repaired, troubleshooting is completed. - If the vehicle is not repaired or additional diagnostic information is not available, reprogram the PCM if a later calibration is available. Retest.