#
REAR WIPER MOTOR REMOVAL/INSTALLATION [5HB]

id0919004755a3

1. Disconnect the negative battery cable.

2. Remove the rear wiper arm and blade. (See REAR WIPER ARM AND BLADE REMOVAL/INSTALLATION [5HB].)

3. Remove the liftgate lower trim. (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION [5HB].)

4. Remove in the order indicated in the table.

1 | Connector
2 | Outer bushing
3 | Bolt
4 | Rear wiper motor

5. Install in the reverse order of removal.

6. Adjust the rear wiper arm and blade. (See REAR WIPER ARM AND BLADE ADJUSTMENT [5HB].)