#
ELECTRONIC CONTROL SYSTEM STRUCTURAL VIEW [JA5AX-EL]

id051705104400
• The TCM control the automatic transaxle operations. The TCM outputs a control signal to the transaxle according to the signal from other sensors and/or switches.

.

1 | TCM
2 | PCM
3 | Selector lever
4 | M range switch
5 | Up switch
6 | Down switch
7 | DLC-2
8 | Brake light switch
9 | AT warning light
10 | Selector indicator light
11 | Gear position indicator light

.

12 | Solenoid valve
13 | TFT sensor
14 | TR switch
15 | Input/turbine speed sensor
16 | Intermediate sensor
17 | VSS
18 | Oil cooler