#
THROTTLE BODY FUNCTION [L3 Turbo]

id0113b5101500
• A throttle body with a single, electronic-control, motor-operated valve has been adopted in place of the previous cable-controlled throttle valve type.
• The PCM determines the throttle valve opening angle based on driving conditions, and operates the motor accordingly.
• The throttle valve opening angle is feedback to the PCM by the TP sensor.