#
SHIFT CONTROL OUTLINE [JA5AX-EL]

id051705689900

## Features

• The TCM selects and determines the shift diagram based on the results of the range and driving mode judgements. Then, based on the shift diagram, the TCM sends the signal to the duty-cycle type solenoid valves and the ON/OFF type solenoid valves, according to the VSS signal and the throttle opening signal, to perform shifting.

## Construction (System Diagram)

.

1 | TR switch
2 | Starter
3 | PCM
4 | CAN
5 | Throttle opening signal
6 | Down switch
7 | Up switch
8 | M range switch
9 | TFT sensor
10 | Shift diagram
11 | Shift solenoid A
12 | Shift solenoid B
13 | Shift solenoid C
14 | VSS
15 | Vehicle speed
16 | Throttle opening angle
17 | TCM