CYLINDER HEAD DISASSEMBLY (II)

id011000500500

1. Disassemble in the order indicated in the table.

e6u110zeb014

1 | Engine hanger
2 | Valve keeper (See Valve Keeper Disassembly Note.)
3 | Upper valve spring seat
4 | Valve spring
5 | Valve
6 | Valve seal (See Valve Seal Disassembly Note.)
7 | Water outlet case

Valve Keeper Disassembly Note

1. Remove the valve keeper using the SSTs.

b3e0110e124

Valve Seal Disassembly Note

1. Remove the valve seal using the SST.

b3e0110e061