#
DTC TABLE

id080200800600
• DTCs are common for present and past malfunction diagnosis.

  Note

  • When DTCs not shown in the DTC table are displayed, replace the SAS control module.
  • If the air bag system warning light does not illuminate or remains illuminated when the ignition switch is turned to the ON position, inspect and repair the air bag system warning light circuit, and then confirm that the air bag system warning light is operational.
  • The air bag system warning light flashes the DTC pattern for five cycles, and then remains illuminated until the ignition switch is turned to the LOCK position.
  • If the SAS control module configuration is performed while the SRS air bag system circuit has a malfunction, the air bag system warning light flashes. Verify that the warning light goes out approx. 15 s after the system circuit malfunction is solved.

DTC | System malfunction location | Page
--- | --- | ---
WDS display | Air bag system warning light
Flashing pattern | Priority ranking
B1017 | 14 |  | 4 | Deployment prohibited because configuration is not set | (See DTC B1017.)
B1231 | 13 |  | 3 | SAS control module activation (deployment) control freeze | (See DTC B1231.)
B1317 | - | Air bag system warning light is illuminated all the time | - | The SAS control module power supply voltage increases (16.1 V or more) | (See DTC B1317, B1318.)
B1318 | - | Air bag system warning light is illuminated all the time | - | The SAS control module power supply voltage decreases (less than 9 V) | (See DTC B1317, B1318.)
B1342 | 12 |  | 2 | SAS control module | (See DTC B1342.)
- | Air bag system warning light is illuminated all the time | 1 | SAS control module (air bag system warning light DTC 12 is displayed)
B1869 | - | Air bag system warning light is illuminated all the time | 1 | Air bag system warning light system circuit open | (See DTC B1869, B1870.)
- | Air bag system warning light is illuminated dose not illuminate | - | Air bag system warning light system circuit short to ground
B1870 | - | Air bag system warning light is illuminated all the time | 1 | Air bag system warning light system circuit short to power supply
B1877 | 33 |  | 13 | Driver-side pre-tensioner seat belt circuit resistance high | (See DTC B1877, B1878, B1879, B1885.)
B1878 | Driver-side pre-tensioner seat belt circuit short to power supply
B1879 | Driver-side pre-tensioner seat belt circuit short to ground
B1881 | 34 |  | 12 | Passenger-side pre-tensioner seat belt circuit resistance high | (See DTC B1881, B1882, B1883, B1886.)
B1882 | Passenger-side pre-tensioner seat belt circuit short to power supply
B1883 | Passenger-side pre-tensioner seat belt circuit short to ground
B1884 | 18 |  | 20 | Passenger air bag deactivation (PAD) indicator circuit open or short to body ground | (See DTC B1884, B1890.)
B1885 | 33 |  | 13 | Driver-side pre-tensioner seat belt circuit resistance low | (See DTC B1877, B1878, B1879, B1885.)
B1886 | 34 |  | 12 | Passenger-side pre-tensioner seat belt circuit resistance low | (See DTC B1881, B1882, B1883, B1886.)
B1890 | 18 |  | 20 | Passenger air bag deactivation (PAD) indicator circuit short to power supply | (See DTC B1884, B1890.)
B1913 | 19 |  | 11 | Driver-side air bag module circuit short to body ground | (See DTC B1913, B1916, B1932, B1934.)
21 |  | 10 | Passenger-side air bag module circuit short to body ground | (See DTC B1913, B1925, B1933, B1935.)
B1916 | 19 |  | 11 | Driver-side air bag module circuit short to power supply | (See DTC B1913, B1916, B1932, B1934.)
B1925 | 21 |  | 10 | Passenger-side air bag module circuit short to power supply | (See DTC B1913, B1925, B1933, B1935.)
B1932 | 19 |  | 11 | Driver-side air bag module circuit resistance high | (See DTC B1913, B1916, B1932, B1934.)
B1933 | 21 |  | 10 | Passenger-side air bag module circuit resistance high | (See DTC B1913, B1925, B1933, B1935.)
B1934 | 19 |  | 11 | Driver-side air bag module circuit resistance low | (See DTC B1913, B1916, B1932, B1934.)
B1935 | 21 |  | 10 | Passenger-side air bag module circuit resistance low | (See DTC B1913, B1925, B1933, B1935.)
B1992 | 22 |  | 15 | Driver-side side air bag module circuit short to power supply | (See DTC B1992, B1993, B1994, B1995.)
B1993 | Driver-side side air bag module circuit short to ground
B1994 | Driver-side side air bag module circuit resistance high
B1995 | Driver-side side air bag module circuit resistance low
B1996 | 23 |  | 14 | Passenger-side side air bag module circuit short to power supply | (See DTC B1996, B1997, B1998, B1999.)
B1997 | Passenger-side side air bag module circuit short to ground
B1998 | Passenger-side side air bag module circuit resistance high
B1999 | Passenger-side side air bag module circuit resistance low
B2228 | 19 |  | 11 | Driver-side air bag module assembly incorrect | (See DTC B2228, B2230, B2232, B2234.)
B2230
B2232
B2234
B2229 | 21 |  | 10 | Passenger-side air bag module assembly incorrect | (See DTC B2229, B2231, B2233, B2235.)
B2231
B2233
B2235
B2444 | 43 |  | 8 | Driver-side side air bag sensor system (internal circuit disabled) | (See DTC B2444, U2017.)
B2445 | 44 |  | 7 | Passenger-side side air bag sensor system (internal circuit disabled) | (See DTC B2445, U2018.)
B2477 | 54 |  | 5 | Configuration error | (See DTC B2477.)
B2773 | 24 |  | 17 | Driver-side curtain air bag module circuit resistance low | (See DTC B2773, B2774, B2775, B2776.)
B2774 | Driver-side curtain air bag module circuit resistance high
B2775 | Driver-side curtain air bag module circuit short to ground
B2776 | Driver-side curtain air bag module circuit short to power supply
B2777 | 25 |  | 16 | Passenger-side curtain air bag module circuit resistance low | (See DTC B2777, B2778, B2779, B2780.)
B2778 | Passenger-side curtain air bag module circuit resistance high
B2779 | Passenger-side curtain air bag module circuit short to ground
B2780 | Passenger-side curtain air bag module circuit short to power supply
B2867 | 31 |  | 6 | Poor connection of any SAS control module connectors | (See DTC B2867.)
U2017 | 43 |  | 8 | Driver-side side air bag sensor (communication error) | (See DTC B2444, U2017.)
U2018 | 44 |  | 7 | Passenger-side side air bag sensor (communication error) | (See DTC B2445, U2018.)