#
REAR DOOR GARNISH INSTALLATION

id091600445900

  Note

  • Double-sided adhesive tape has already been attached to the new rear door garnish.

  Warning

  • Using a razor with bare hands can cause injury. Always wear gloves when using a razor.

1. When installing a new rear door garnish, follow the procedure below:

  (1) Remove the adhesive remaining on the body using razor.
  (2) Remove any grease or dirt from the adhesion surface of the body.

2. When reusing the rear door garnish, follow the procedure below:

  (1) Remove the adhesive remaining on the rear door garnish and the body using a razor.
  (2) Remove any grease or dirt from the adhesion surface of the rear door garnish and the body.
  (3) Apply primer to the bonding area of the rear door garnish.
  (4) Attach double-sided adhesive tape to the rear door garnish as shown.

3. Peel off the backing of the double-sided adhesive tape, then install the rear door garnish to the body.