#
DRIVELINE/AXLE SPECIFICATIONS

id030000100200

2WD

Item | Specification
--- | ---
Engine | L8, LF, L3 | MZR-CD (RF Turbo)
Front axle | Bearing type | Angular ball bearing
Rear axle | Bearing type | Angular ball bearing
Drive shaft | Joint type | Wheel side | Bell joint
Differential side | ATX: Tripod joint MTX: Double offset joint | Double offset joint
Shaft diameter | (mm {in}) | 26.0 {1.02} | 30.0 {1.18}
Joint shaft | Shaft diameter | (mm {in}) | 26.0 {1.02} | 36.0 {1.42}

4WD

Item | Specification
--- | ---
Engine | L3 | L3 Turbo
Front axle | Bearing type | Angular ball bearing
Rear axle | Bearing type | Angular ball bearing
Front drive shaft | Joint type | Wheel side | Bell joint
Differential side | Tripod joint | Double offset joint
Shaft diameter | (mm {in}) | 25.0 {0.98} | 27.0 {1.06}
Joint shaft | Shaft diameter | (mm {in}) | 29.0 {1.14} | 28.0 {1.10}
Rear drive shaft | Joint type | Wheel side | Bell joint
Differential side | Double offset joint
Shaft diameter | (mm {in}) | 24.0 {0.94}
Rear and front wheel torque distribution unit | Electronic control coupling
Rear differential | Reduction gear | Hypoid gear
Differential gear | Straight bevel gear
Ring gear size | (Inches) | 6.5 | 7.4
Final gear ratio | 2.928
Gears: Number of teeth | Drive pinion | 14
Ring gear | 41
Differential oil | Type | Grade | API service GL-5
Viscosity | SAE 80W-90
Amount (Approximate quantity) | (L {US qt, lmp qt}) | 1.0 {1.1, 0.9}

Propeller shaft

Item | Specification
--- | ---
Transaxle type | A26MX-R | JA5AX-EL
Length | (mm {in}) | L1 | 728 {28.66} | 720.5 {28.37}
L2 | 750 {29.53} | 735.0 {28.94}
L3 | 454 {17.87} | 503.0 {19.80}
Outer diameter | (mm {in}) | D1 | 60.5 {2.38} | 57.0 {2.24}
D2 | 60.5 {2.38} | 57.0 {2.24}
D3 | 60.5 {2.38} | 57.0 {2.24}
Joint type | Constant velocity joint and cross-shaped joint | Tripod joint, Universal joint
Tripod joint | Double offset joint | Double offset joint

Transfer

Item | Specification
--- | ---
Transaxle type | A26MX-R | JA5AX-EL
Transfer oil | Type | SAE 80W-90 API Service GL-5
Capacity (approximate quantity) (L {US qt, Imp qt}) | 1.2 {1.3,1.1} | 0.62 {0.66, 0.55}