#
HIGH-MOUNT BRAKE LIGHT REMOVAL/INSTALLATION

id091800802000

## 4SD

### In-vehicle-type

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Connector
2 | High-mount brake light
3 | Socket
4 | High-mount brake light bulb

3. Install in the reverse order of removal.

### Rear spoiler type

1. Disconnect the negative battery cable.

2. Remove the rear spoiler. (See REAR SPOILER REMOVAL/INSTALLATION [4SD, 5HB].)

3. Remove in the order indicated in the table.

1 | Nut
2 | Bracket
3 | Bolt
4 | High-mount brake light

4. Install in the reverse order of removal.

## 5HB

1. Disconnect the negative battery cable.

2. Remove the liftgate lower trim. (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION [5HB].)

3. Remove in the order indicated in the table.

1 | Connector
2 | Nut
3 | High-mount brake light
4 | Lens
5 | Socket
6 | High-mount brake light bulb

4. Install in the reverse order of removal.

## WGN

### In-vehicle-type

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION [WGN].)

3. Remove in the order indicated in the table.

1 | Connector
2 | Socket
3 | High-mount brake light bulb
4 | High-mount brake light

4. Install in the reverse order of removal.

### Rear spoiler type

1. Disconnect the negative battery cable.

2. Remove the rear spoiler. (See REAR SPOILER REMOVAL/INSTALLATION [WGN].)

3. Remove in the order indicated in the table.

1 | Bolt
2 | Cover
3 | Connector
4 | High-mount brake light

4. Install in the reverse order of removal.