PCM REMOVAL/INSTALLATION [L8, LF, L3]

id0140a5802400

  Note
  • When replacing the PCM, perform the following:
    ― PCM configuration (See PCM CONFIGURATION [L8, LF, L3].)
    ― Immobilizer system-related part programming (See IMMOBILIZER SYSTEM REPROGRAM PROCEDURE [KEYLESS ENTRY SYSTEM].)(See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING [WITH ADVANCED KEYLESS SYSTEM].)

1. Disconnect the negative battery cable.

2. For R.H.D., perform the following procedures.

  (1) Remove the front side trim (left-side).

  (2) Partially peel back the flower covering.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

R.H.D.

am6zzw00011888

1 | PCM cover No. 1 (See Set Bolt Removal Note.) (See Set Bolt Installation Note.)
2 | PCM cover No. 2
3 | PCM connector
4 | PCM

L.H.D.

am6zzw00011889

1 | PCM connector
2 | PCM

Set Bolt Removal Note

1. Using a chisel and a hammer, cut a groove on the head of the set nut/bolt so that a screwdriver can be inserted.

2. Loose the set nut/bolt using an impact screwdriver or pliers.

am6zzw00011890

Set Bolt Installation Note

1. Install a new set nut/bolt and tighten it until the neck of the nut/bolt is cut.

am6zzw00011891