#
HEADLIGHT LEVELING SWITCH REMOVAL/INSTALLATION

id091800464200

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Headlight leveling switch (See Headlight Leveling Switch Removal Note.)
2 | Connector

3. Install in the reverse order of removal.

## Headlight Leveling Switch Removal Note

1. Insert your hand from the lower side of the dashboard and squeeze the tabs of the headlight leveling switch.

2. Pull the headlight leveling switch forward to remove it.