#
NO.21 NOISE OCCURS AT IDLE WHEN VEHICLE IS STOPPED IN D RANGE, OR IN R POSITION [JA5AX-EL]

id050305802600

21 | Noise occurs at idle when vehicle is stopped in D range, or in R position
DESCRIPTION | • Transaxle noisy in driving ranges when vehicle idling.
POSSIBLE CAUSE | • Although the malfunction is basically the same as No.20 "Noise occurs at idle when vehicle is stopped in all positions/ranges", other causes may be selector lever position disparity or TR switch position disparity. Note • Before following troubleshooting steps, make sure that Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.