#
WARNING/GUIDANCE FUNCTION OPERATION

id0914b5102800
• If the system is operated impropeLRy, it warns the driver using the indicator light in the instrument cluster, buzzer sound, and keyless buzzer in the driver's side front fender panel.
• The operation condition of the actuator is indicated by the indicator light and buzzer sound to guide user's operation.

Item | Operation condition | Keyless buzzer (outside the vehicle) | Instrument cluster
--- | --- | --- | ---
Buzzer (Interior) | Keyless warning light (red) | Keyless indicator light (green)
Warning | Start knob not in LOCK warning | Driver's door is open with start knob in ACC position | - | Sounds 6 times | - | -
Card key out of vehicle warning*1 | Card key cannot be detected inside vehicle with driver's door open and start knob not in LOCK position | - | Sounds 3 times*2 | Flashes*4 | -
Card key cannot be detected inside vehicle with all doors closed and start knob not in LOCK position | Sounds 3 times | - | Flashes*4 | -
Card key cannot be detected inside vehicle with start knob not in LOCK position and under any condition other than above | - | - | Flashes*4 | -
Door lock inoperable warning | Request switch is pressed from outside vehicle with proper card key inside vehicle and another card key carried | Sounds 3 times | - | - | -
Request switch is pressed with card key is carried and a door open or start knob not in LOCK position | Sounds 3 times | - | - | -
Battery voltage low indication | Card key battery voltage depleted | - | - | - | Flashes (Approx. 30 s after IG OFF)
Guidance | Start knob operable guidance | Start knob is operable (lock released) when it is pressed | - | - | - | On (Max. 3 s)
Start knob inoperable guidance | Start knob is inoperable (locked) when it is pressed | - | - | Flashes | -
Lock/unlock answer back | Doors are locked/unlocked with normal/advanced keyless entry function | Locked: Once Unlocked: Twice | - | - | -

  *1 :
If the start knob is turned to the LOCK position with the card key out of the vehicle, the start knob is inoperable(the engine cannot be restarted). For vehicles with the immobilizer system, the engine cannot be restarted by turning the start knob from the ACC position to the START position even though the start knob has not been turned to the LOCK position.
  *2 :
When the ignition switch is off (except for LOCK position), "Start knob not in LOCK warning" (buzzer sound) overrides.
  *3 :
Initial setting is OFF.
  *4 :
Stops flashing and goes out if the card key is detected inside the vehicle.