#
FRONT AND REAR FOG LIGHT SWITCH INSPECTION

id091800805200

## Light switch LH side

1. Remove the light switch. (See LIGHT SWITCH REMOVAL/INSTALLATION.)

2. Inspect for continuity between the light switch terminals using a tester.

  • If there is any malfunction, replace the light switch.

## Light switch RH side

1. Remove the light switch. (See LIGHT SWITCH REMOVAL/INSTALLATION.)

2. Inspect for continuity between the light switch terminals using a tester.

  • If there is any malfunction, replace the light switch.