#
SIMULATION FUNCTION [FS5A-EL]

id050221100800
• By using the WDS or equivalent, simulation items for input/output parts preset in the TCM can be optionally selected and operated regardless of TCM control conditions.

## Simulation Item Table

X: Available

Simulation item | Applicable component | Unit/Condition | Operation | TCM terminal
--- | --- | --- | --- | ---
IG ON | Idle
LPS | Pressure control solenoid control A signal in TCM | % |  | X | 1E 1G
LPS B | Pressure control solenoid control B signal in TCM | % |  | X | 1D
SSA/SS1 | Shift solenoid A control signal in TCM | % |  | X | 1A
SSB/SS2 | Shift solenoid B control signal in TCM | % |  | X | 1B
SSC/SS3 | Shift solenoid C control signal in TCM | % |  | X | 1C
SSD/SS4 | Shift solenoid D control signal in TCM | On/Off |  | X | 1F
SSE_SS5 | Shift solenoid E control signal in TCM | On/Off |  | X | 1H
SSF_SS6 | Shift solenoid F control signal in TCM | On/Off |  | X | 1J